The allocation of failure detection rate and failure isolation rate is performed using the following formulas:





Where,

, —the allocation result of the ith component.

, —value to be allocated.

—failure rate of system.

—failure rate of ith component.

—detected failure rate of system ().

—detected failure rate of ith component ().

—number of ith component.